# High Priority Traffic

Use this option to monitor high priority traffic reception statistics from physical medium-dependent layer for current interval of a particular side of a particular SRP interface.

## Procedure

To access high priority information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Media dependent Current Interval Statistics dialog box appears.

2. Select Rx Physical Layer Statistics from the Category menu to display physical layer statistics reception information.

3. Select High Priority Traffic from the Category menu to display high priority traffic information.

High Priority Traffic dialog box displays:

Unicast High Priority Packets (SrpRingCurUcastHighPriPktsIn)

Unicast High Priority Octets (SrpRingCurUcastHighPriOctetsIn)

Multicast High Priority Packets (SrpRingCurMcastHighPriPktsIn)

Multicast High Priority Octets (SrpRingCurMcastHighPriOctetsIn)

### Unicast High Priority Packets (SrpRingCurUcastHighPriPktsIn)

Number of high-priority unicast packets received from physical medium-dependent layer during a 15-minute interval.

### Unicast High Priority Octets (SrpRingCurUcastHighPriOctetsIn)

Number of high-priority unicast octets received from physical medium-dependent layer during a 15-minute interval.

### Multicast High Priority Packets (SrpRingCurMcastHighPriPktsIn)

Number of high-priority multicast packets received from physical medium-dependent layer during a 15-minute interval.

### Multicast High Priority Octets (SrpRingCurMcastHighPriOctetsIn)

Number of high-priority multicast octets received from physical medium-dependent layer during a 15-minute interval.

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components