# RSVP Specific Attributes

The table displays the following information:

> UDP neighbors

> IP neighbors

> Total neighbors

> RSVP Enable

> UDP Encapsulation

> RSVP Value Kb

> RSVP Value K

> Time to Live

> Refresh Message Interval

### UDP neighbors (rsvpIfUdpNbrs )

Indicates the number of neighbors perceived to be using only the RSVP UDP encapsulation.

### IP neighbors (rsvpIfIpNbrs )

Indicates the number of neighbors perceived to be using only the RSVP IP encapsulation.

### Total neighbors (rsvpIfNbrs )

Indicates the total number of neighbors currently perceived to be using any kind of encapsulation. The number of total neighbors will exceed rsvpIfIpNbrs + rsvpIfUdpNbrs by the number of neighbors using both encapsulations.

### RSVP Enable (rsvpIfEnabled )

Inidcates the RSVP status on an interface.

Value | Description
True | RSVP is enabled on the interface.
False | RSVP is not enabled on the interface.

### UDP Encapsulation (rsvpIfUdpRequired )

Indicates UDP encapsulation status.

Value | Description
True | Manual configuration forces the uses of UDP encapsulation on the interface.
False | UDP encapsulation is only used if rsvpIfUdpNbrs is not zero.

### RSVP Value Kb (rsvpIfRefreshBlockadeMultiple )

Indicates the minimum number of refresh intervals that a blockade state will last once it is entered.

### RSVP Value K (rsvpIfRefreshMultiple )

Indicates the minimum number of refresh intervals that must elapse before a PATH or RESV message not being refreshed will be aged out

### Time to Live (rsvpIfTTL)

Indicates the value of SEND_TTL used on an interface for the message the node originates. If the value is set to zero, the node determines the TTL.

### Refresh Message Interval (rsvpIfRefershInterval )

(units: milliseconds)

Indicates the minimum period between refresh transmission of a given PATH or RESV message on an interface.