# RP Update Statistics Contd

1. Right-click on the MWAM Card and select Configure.
2. Select category MWAM module.
3. Select a row and click the Statistics button.
4. Select category CDMA PDSN PCF & SO Based Statistics.
5. Select a row and click on the RP Update Statistics button and from the Category select RP Update Statistics Contd.

The following information appears:

> Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdPcfHandoffs)

> Unacknowledged Registration Updates (cCdmaSoRpUpdHandoffNotAckedReqs)

> Acknowledged Registration Updates (cCdmaSoRpUpdHandoffReceivedAcks)

> Accepted Registration Updates (cCdmaSoRpUpdHandoffAcceptedReqs)

> Denied Registration Updates (cCdmaSoRpUpdHandoffDeniedReqs)

> Acknowledgements Discarded (cCdmaSoRpUpdHandoffDiscardedAcks)

> Initial Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdHandoffInitTxdReqs)

> Initial Retransmitted Update Registrations (cCdmaSoRpUpdHandoffReTxdReqs)

### Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdPcfHandoffs)

Number of update registrations sent as a result of inter PCF handoffs since the system was last restarted.

### Unacknowledged Registration Updates (cCdmaSoRpUpdHandoffNotAckedReqs)

Total number of A11 Registration Updates (sent as the result of inter PCF handoffs), for which no corresponding A11 Registration Acknowledgements have been received since the system was last restarted.

### Acknowledged Registration Updates (cCdmaSoRpUpdHandoffReceivedAcks)

Total number of A11 Registration Acknowledgements received for the A11 Registration Updates that were sent as the result of inter PCF handoffs since the system was last restarted.

### Accepted Registration Updates (cCdmaSoRpUpdHandoffAcceptedReqs)

Total number of A11 Registration Acknowledgements received with the Status field set to zero, which indicates that the corresponding Registration Update was accepted, since the system was last restarted.

### Denied Registration Updates (cCdmaSoRpUpdHandoffDeniedReqs)

Total number of A11 Registration Acknowledgements received with the Status field set to non-zero, which indicates that the corresponding Registration Update was denied, since the system was last restarted.

### Acknowledgements Discarded (cCdmaSoRpUpdHandoffDiscardedAcks)

Total number of A11 Registration Acknowledgements discarded since the system was last restarted.

### Initial Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdHandoffInitTxdReqs)

Total number of initial A11 Registration Updates sent as the result of inter PCF handoffs, excluding the re-transmitted A11 Registration Updates, since system was last restarted.

### Initial Retransmitted Update Registrations (cCdmaSoRpUpdHandoffReTxdReqs)

Total number of re-transmitted A11 Registration Updates sent because the initial Registration Update (sent as a result of inter PCF handoffs) was not acknowledged or denied since the system was last restarted.