# Receive Side Physical Layer Errors

Use this option to monitor error statistics of traffic from layer 1 physical medium in a particular interval for a particular side of a particular SRP interface.

## Procedure

To access receive side physical layer error information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Error Statistics dialog box appears.

2. Select Rx Physical Layer Errors from the Category menu to display receive side physical layer error information.

Rx Physical Layer Errors dialog box displays:

Data Parity Error (srpRingIntRxErrorsDataParity)

Short Packets (srpRingIntRxErrorsShortPackets)

Giant Packets (srpRingIntRxErrorsGiantPackets)

Bad Packets (srpRingIntRxErrorsSideBadPackets)

CRC Error Packets (srpRingIntRxErrorsCRC)

### Data Parity Error (srpRingIntRxErrorsDataParity)

Number of data parity errors received from layer-1 physical medium during a 15-minute interval in the past 24 hours.

### Short Packets (srpRingIntRxErrorsShortPackets)

Number of short packets received from layer-1 physical medium during a 15-minute interval in the past 24 hours.

### Giant Packets (srpRingIntRxErrorsGiantPackets)

Number of giant packets received from layer-1 physical medium during a 15-minute interval in the past 24 hours.

### Bad Packets (srpRingIntRxErrorsSideBadPackets)

Number of bad packets received from layer-1 physical medium during a 15-minute interval in the past 24 hours.

### CRC Error Packets (srpRingIntRxErrorsCRC)

Number of packets with CRC errors received from layer-1 physical medium during a 15-minute interval in the past 24 hours.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components