# GGSN CSG Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select GGSN CSG Statistics from the Category list.

The following information appears:

> Outbound Packets Sent (cGgsnSACsgOutboundMsgs)

> Outbound Octets Sent (cGgsnSACsgOutboundOctets)

> Inbound Packets Received (cGgsnSACsgInboundMsgs)

> Inbound Octets Received (cGgsnSACsgInboundOctets)

> Initial Quota Grant (cGgsnSACsgServiceAuthReqs)

> Service Authorization Request (cGgsnSACsgServiceAuthResps)

> Service Re-Authorization Request (cGgsnSACsgServiceReAuthReqs)

> CSG Quota Return Messages (cGgsnSACsgQuotaReturns)

### Outbound Packets Sent (cGgsnSACsgOutboundMsgs)

The aggregate number of echo request, echo response, and node alive messages sent.

### Outbound Octets Sent (cGgsnSACsgOutboundOctets)

The aggregate number of echo request, echo response, and node alive messages sent in terms of octets.

### Inbound Packets Received (cGgsnSACsgInboundMsgs)

The aggregate number of echo request, echo response, and node alive messages received.

### Inbound Octets Received (cGgsnSACsgInboundOctets)

The aggregate number of echo request, echo response, and node alive messages received in terms of octets.

### Initial Quota Grant (cGgsnSACsgServiceAuthReqs)

The number of requests by the Content Service Gateway for an initial quota grant of a particular category. The Content Service Gateway allows only synchronous quota grants (that is, grants due to explicit requests from it).

### Service Authorization Request (cGgsnSACsgServiceAuthResps)

The number of responses given to the Content Service Gateway for service authorization requests.

### Service Re-Authorization Request (cGgsnSACsgServiceReAuthReqs)

Indicates the number of service reauthorization requests by the Content Service Gateway for a category verification.

### CSG Quota Return Messages (cGgsnSACsgQuotaReturns)

The number of quota return messages from the Content Service Gateway. The Content Service Gateway sends a quota return message when the validity timer expires or there is no response message from the quota server. On receipt of quota return message, the quota server returns the usage of a particular category.