# SSG General Information

This dialog box displays general information on the Service Selection Gateway (SSG).

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select SSG General Information from the Category list.

The following information is displayed:

> Time Interval (cssgCfgAutoLogOffInterval)

> ICMP Ping Retries (cssgCfgAutoLogOffIcmpRetries)

> Maximum Service (cssgCfgMaxServicesPerUser)

> Default Ip Address Type (cssgCfgDefaultNetWorkType)

> Default Ip Address (cssgCfgDefaultNetWork)

> Access Request Receipt Port (cssgCfgRadiusAuthenPort)

> Accounting Receipt Port (cssgCfgRadiusAccountingPort)

> Authenticated TCP Group (cssgCfgTCPRedirGrpForUnAuthUsers)

> Unauthorized TCP Group (cssgCfgTCPRedirGrpForUnAuthServ)

> SMTP TCP Group (cssgCfgTcpRedirGrpForSMTP)

> Initial Captivation TCP Group (cssgCfgTcpRedirGrpForInitialCapt)

> Advertising Captivation TCP Group (cssgCfgTcpRedirGrpForAdvCapt)

### Time Interval (cssgCfgAutoLogOffInterval)

Interval at which connectivity to a host is checked.

If the host is not reachable, SSG logs off the host if the auto-logoff feature is enabled.

### ICMP Ping Retries (cssgCfgAutoLogOffIcmpRetries)

Number of ICMP ping attempts made by SSG to check connectivity to a host.

### Maximum Service (cssgCfgMaxServicesPerUser)

Maximum number of services allowed per user.

### Default Ip Address Type (cssgCfgDefaultNetWorkType)

Type of the IP address stored in cssgCfgDefaultNetwork.

### Default Ip Address (cssgCfgDefaultNetWork)

IP address or subnet that users can access without authentication. This is the address where the Cisco service selection dashboard or subscriber-edge service manager resides.

### Access Request Receipt Port (cssgCfgRadiusAuthenPort)

Port on which SSG receives access request packets from remote authentication dial-in user service clients.

### Accounting Receipt Port (cssgCfgRadiusAccountingPort)

Port on which SSG receives accounting packets from remote authentication dial-in user service clients.

### Authenticated TCP Group (cssgCfgTCPRedirGrpForUnAuthUsers)

TCP redirect group to which SSG directs unauthenticated users.

### Unauthorized TCP Group (cssgCfgTCPRedirGrpForUnAuthServ)

TCP redirect group to which SSG directs unauthorized service access users.

### SMTP TCP Group (cssgCfgTcpRedirGrpForSMTP)

TCP redirect group to which SSG redirects SMTP traffic.

### Initial Captivation TCP Group (cssgCfgTcpRedirGrpForInitialCapt)

TCP redirect group for initial captivation.

### Advertising Captivation TCP Group (cssgCfgTcpRedirGrpForAdvCapt)

TCP redirect group for advertising captivation.