# Content Switching Module - CSM Configuration

The CSM Configuration dialog displays details of the CSM VLANs.

## Navigation

1. Right-click the Content Switching Module, then select CSM Configuration ....

The following information appears:

VLAN ID

VLAN Type

IP Address

Subnet Mask

Gateway

From the CSM Configuration dialog box:

Click Create to create new SLB VLANs.

Selet a row in the table and click Delete to delete the selected VLAN. You can delete the entire VLAN, the IP address, or the Gateway.

To modify the IP address, or the subnet mask, or both, select a row, then click Modify.

## CLI Commands

To display the details of SLB VLANs associated with the CSM blade, type the following command:

sh ip slb vlan

The command for deleting SLB VLAN is:

module ContentSwitchingModule <slotNo>, VLAN <vlan> [client | server], no gateway <addr> and no ip address <addr><mask>

### VLAN ID

Number assigned to a particular VLAN.

### VLAN Type

Type shows if the VLAN resides on a client or a server.

### IP Address

IP address associated with a particular VLAN.

### Subnet Mask

IP mask address associated with a particular VLAN.

### Gateway

IP gateway for the traffic in a particular VLAN.