# CDMA PDSN Status Change Statistics

This dialog box is applicable to Member and Peer to Peer clusters. It displays the status change statistics for the packet data serving node (PDSN).

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Status Change Statistics.

### IS to OOS change (cCdmaStatusIS2OOSes)

Total number of changes from in service (IS) to out of service (OOS).

### OOS to IS change (cCdmaStatusOOS2ISes)

Total number of changes from OOS to IS.