# Information of Mobile Networks Associated with Home Agent

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module. Select a row and click the Configure button.

3. Select category Information of Mobile Networks associated with HA.

The following information appears:

> Mobile Network Address Type (cmiHaMobNetAddressType)

> Mobile Network IP Address (cmiHaMobNetAddress)

> Mobile Network Prefix Length (cmiHaMobNetPfxLen)

> Dynamic Registration Status (cmiHaMobNetDynamic)

> Create/Delete Row (cmiHaMobNetStatus)

### Mobile Network Address Type (cmiHaMobNetAddressType)

Type of IP address stored in cmiHaMobNetAddress. Only IPv4 address type is supported.

### Mobile Network IP Address (cmiHaMobNetAddress)

IP address of the mobile network. Only IPv4 addresses are supported.

### Mobile Network Prefix Length (cmiHaMobNetPfxLen)

Prefix length associated with the mobile network IP address.

### Dynamic Registration Status (cmiHaMobNetDynamic)

Indicates whether the mobile network has been registered dynamically or not.

### Create/Delete Row (cmiHaMobNetStatus)

The row status for the mobile network entry.