# Temperature Status

The Temperature Status dialog monitors the temperature of Network Processing Engine (NPE-G100) or Network Services Engine (NSE-100) on a CISCO 7304 device.

## Procedure

1. Right-click the chassis, then select Monitor.

2. Select Temperature Status from the drop-down list.

The temperature is measured at various test points.

The test points on NSE are:

- NSE outlet (NSE outlet)

- NSE inlet (NSE inlet)

- NSE hotspot (NSE hotspot)

- NSE db (NSE db)

The test points on NPE-G100 are:

- NPE-G100 outlet ( NPE-G100 outlet )

- NPE-G100 inlet ( NPE-G100 inlet )

- NPE-G100 hotspot ( NPE-G100 hotspot )