# CDMA PDSN A11 Registration Denial Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select CDMA PDSN A11 Registration Denial Statistics from the Category list.

The following information appears:

> Denied A11 for De-established R-P Conn (cCdmaRpDeRegHandoffDeniedReqs)

> Denied Initial A11 Registration Req (cCdmaRpInitRegDiscardedReqs)

> Discarded A11 Re- Registration Req (cCdmaRpReRegDiscardedReqs)

> A11 De-Registration Req Discarded (cCdmaRpDeRegDiscardedReqs)

> Denied Handoff A11 Registration Req (cCdmaRpHandoffRegDeniedReqs)

> Discarded Handoff A11 Registration Req (cCdmaRpHandoffRegDiscardedReqs)

> Active PCF Handoffs (cCdmaRpInterPCFActiveHandoffs)

> Dormant PCF Handoffs (cCdmaRpInterPCFDormantHandoffs)

### Denied A11 for De-established R-P Conn (cCdmaRpDeRegHandoffDeniedReqs)

The total number of denied A11 Registration Requests meant for de-establishing the R-P connections with the Packet Control Function (PCF) from which the mobile node was handed off since the system was last restarted. The Code field in the corresponding Registration Reply message is set to non-zero.

### Denied Initial A11 Registration Req (cCdmaRpInitRegDiscardedReqs)

The number of Initial A11 Registration Requests silently discarded since the system was last restarted.

### Discarded A11 Re- Registration Req (cCdmaRpReRegDiscardedReqs)

The number of A11 Re-Registration Requests silently discarded since the system was last restarted.

### A11 De-Registration Req Discarded (cCdmaRpDeRegDiscardedReqs)

The number of A11 De-Registration Requests silently discarded since the system was last restarted.

### Denied Handoff A11 Registration Req (cCdmaRpHandoffRegDeniedReqs)

The total number of denied handoff A11 Registration Requests meant for already existing sessions since the system was last restarted.

### Discarded Handoff A11 Registration Req (cCdmaRpHandoffRegDiscardedReqs)

The number of handoff A11 Registration Requests silently discarded since the system was last restarted.

### Active PCF Handoffs (cCdmaRpInterPCFActiveHandoffs)

The number of Inter PCF active handoffs since the system was last restarted.

### Dormant PCF Handoffs (cCdmaRpInterPCFDormantHandoffs)

The number of Inter PCF dormant handoffs since the system was last restarted.