# Receive Side Higher Layer Errors

Use this option to monitor error statistics of traffic from higher layer in a particular interval for a particular side of a particular SRP interface.

## Procedure

To access receive side higher layer error information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Error Statistics dialog box appears.

2. Select Rx Higher Layer Errors from the Category menu to display receive side higher layer error information.

Rx Higher Layer Errors dialog box displays:

Data Parity Error (srpHostIntRxErrorsDataParity)

Short Packets (srpHostIntRxErrorsShortPackets)

Giant Packets (srpHostIntRxErrorsGiantPackets)

Bad Packets (srpHostIntRxErrorsSideBadPackets)

### Data Parity Error (srpHostIntRxErrorsDataParity)

Number of data parity errors received from the higher layer during a 15-minute interval in the past 24 hours.

### Short Packets (srpHostIntRxErrorsShortPackets)

Number of short packets received from the higher layer during a 15-minute interval in the past 24 hours.

### Giant Packets (srpHostIntRxErrorsGiantPackets)

Number of giant packets received from the higher layer during a 15-minute interval in the past 24 hours.

### Bad Packets (srpHostIntRxErrorsSideBadPackets)

Number of bad packets received from the higher layer during a 15-minute interval in the past 24 hours.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components