# IP Addresses and CiscoView Invocation Options

Invoking embedded LS1010/Cat8510-CSR devices from Cat5500:

The latest version of CiscoView’s Catalyst 5500 package can now “remember” embedded LS1010/Cat8510-CSR IP Address in each subsequent invocation of the parent Cat5500 device.

Click on the MultiServiceSwitchRouter icon on the Cat5500 device and the following options are displayed:

LS1010 Host IP Address

Managing a Catalyst 5500 with an LS1010 PAM