# Displaying Device Environment Information

The CiscoView Monitor Device window displays the following environment information:

Airflow Temp In

Airflow Temp Out

+5 Volt

+12 Volt

-12 Volt

+24 Volt

+2.5 Reference

# Airflow Temp In

Displays the current temperature of air entering the router (Cisco 7000).

# Airflow Temp Out

Displays the temperature of the exhaust airflow of the router (Cisco 7000).

# +5 Volt (envTestPt3Measure)

Displays the current value (in millivolts) for the +5V line from the power supply on the router (Cisco 7000).

# +12 Volt (envTestPt4Measure)

Displays the current value (in millivolts) of the +12V line from the power supply of the router.

# -12 Volt (envTestPt5Measure)

Displays the current value (in millivolts) of the -12V line from the power supply of the router.

# +24 Volt (envTestPt6Measure)

Displays the current value (in millivolts) of the +24V line from the power supply of the Cisco 7000 router.

# +2.5 Reference

Displays the current value (in millivolts) of the +2.5 reference line from the power supply.