# GGSN - SGSN Throughput

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select GGSN – SGSN T hroughput from the Category list.

The following information appears:

> Remote Address (cGtpPathAddress)

> Remote Port (cGtpPathPort)

> Collection Interval (cGgsnSgsnThruPutInterval)

### Remote Address (cGtpPathAddress)

An address that uniquely identifies the remote node to which this path is established.

### Remote Port (cGtpPathPort)

Port on the remote node. A value of zero is invalid.

### Collection Interval (cGgsnSgsnThruPutInterval)

One of the values set in the objects cGgsnThruputIntervalOne or cGgsnThruputIntervalTwo, except for value zero (0) which means that throughput collection is disabled.