# CDMA PDSN Addressing Schema Statistics

This dialog box is applicable to Member and Peer to Peer clusters. It displays the handoff statistics of the packet data serving node (PDSN).

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Addressing Schema Statistics.

The following information is displayed:

> Static IP negotiated by Simple Ip (cCdmaAddressStaticSIPs)

> Dynamic IP negotiated by Simple Ip (cCdmaAddressDynamicSIPs)

> Static IP negotiated by MOIP (cCdmaAddressStaticMIPs)

> Dynamic IP negotiated by MOIP (cCdmaAddressDynamicMIPs)

> Static IP negotiated by Proxy MOIP (cCdmaAddressStaticPMIPs)

> Dynamic IP negotiated by Proxy MOIP (cCdmaAddressDynamicPMIPs)

> Static IP negotiated by VPDN (cCdmaAddressStaticVPDNs)

> Dynamic IP negotiated by VPDN (cCdmaAddressDynamicVPDNs)

### Static IP negotiated by Simple Ip (cCdmaAddressStaticSIPs)

Total number of simple IP calls that negotiated static IP addresses.

### Dynamic IP negotiated by Simple Ip (cCdmaAddressDynamicSIPs)

Total number of simple IP calls that negotiated dynamic IP addresses.

### Static IP negotiated by MOIP (cCdmaAddressStaticMIPs)

Total number of mobile IP calls that negotiated static IP addresses.

### Dynamic IP negotiated by MOIP (cCdmaAddressDynamicMIPs)

Total number of mobile IP calls that negotiated dynamic IP addresses.

### Static IP negotiated by Proxy MOIP (cCdmaAddressStaticPMIPs)

Total number of proxy mobile IP calls that negotiated static IP addresses.

### Dynamic IP negotiated by Proxy MOIP (cCdmaAddressDynamicPMIPs)

Total number of proxy mobile IP calls that negotiated dynamic IP addresses.

### Static IP negotiated by VPDN (cCdmaAddressStaticVPDNs)

Total number of VPDN calls that negotiated static IP addresses.

### Dynamic IP negotiated by VPDN (cCdmaAddressDynamicVPDNs)

Total number of VPDN calls that negotiated dynamic IP addresses.