# OSPF ToS Metrics for Nonvirtual Interface

The OSPF ToS Metrics for Nonvirtual Inteface dialog box displays the type of service metrics for a non-virtual interface.

## Procedure

For CiscoView versions earlier than 5.2:

1. Right-click the device. Then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select OSPF from the SelectProtocol list. Then click the Details button. The OSPF Configuration dialog box appears.

4. Select ToS Metrics for Nonvirtual Interface from the Category list.

For CiscoView version 5.2 and later:

1. Right-click the device and then select Configure, or double-click the device.

2. Select Protocols from the Category list.

3. Select OSPF from the SelectProtocol list, then click the Details button. The OSPF Configuration dialog box appears.

   Note: The left frame in the dialog box displays the categories and the right frame displays the category details or a table. If a table is displayed, the variable on which the table is indexed and the key values of the index are listed below the category. Double-click the category to view the table and double-click a key value to view details of a particular row in the table.

   Multiple indexes for a table, if any, are listed below the category in a nested manner. Select a key value to view the rows of the table about that value. Select a key value of the lowest indexing variable to view the details of that particular row.

4. Select ToS Metrics for Nonvirtual Interface from the left pane.

The following information appears:

Interface IP Address (ospfIfMetricIpAddress)

Addressless Interface (ospfIfMetricAddressLessIf)

TOS Metric being Referenced (ospfIfMetricTOS)

Metric for TOS on the Interface (ospfIfMetricMetric)

Metric Entry Valid (ospfIfMetricStatus)

## Related Topics

OSPF Address Range Configuration

OSPF Area Configuration

OSPF General Configuration

OSPF Host Configuration

OSPF Interface Configuration

OSPF Link State Database

OSPF Neighbor Configuration

OSPF Stub Area Configuration

OSPF Virtual Neighbor Configuration

OSPF Virtual Interface Configuration

### Interface IP Address (ospfIfMetricIpAddress)

IP address of the OSPF interface. On row creation, this can be derived from the instance.

### Addressless Interface (ospfIfMetricAddressLessIf)

Eases the instancing of addressed and addressless interfaces. This variable takes the value 0 on interfaces with IP addresses, and the value of ifIndex for interfaces having no IP address. On row creation, this can be derived from the instance.

### TOS Metric being Referenced (ospfIfMetricTOS)

Type of service metric being referenced. On row creation, this can be derived from the instance.

### Metric for ToS on the Interface (ospfIfMetricMetric)

Metric for the type of service on the interface. The default of the ToS 0 Metric is 10^8 / ifSpeed.

The value FFFF means there is no route via this ToS.

### Metric Entry Valid (ospfIfMetricStatus)

Indicates the validity or invalidity of the entry. Setting this object to invalid has the effect of rendering it inoperative. The internal effect (row removal) is implementation dependent.