PIB DSCP Assignment (RED)

# PIB DSCP Assignment (RED)

Device>Configure>PIB>DSCP Assignment (RED)

This table defines a class of lower and upper values for each threshold set in a queue supporting WRED. If the size of the queue for a given threshold is below the lower value, then packets assigned to that threshold are always accepted into the queue. If the size of the queue is above upper value, then packets are always dropped. If the size of the queue is between the lower and the upper, then packets are randomly dropped.

Red (qosIfRedId)

This table field provides an ID to identify the instance of the policy class.

Role (qosIfRedRoles)

This table field provides the role combination the interface must be configured with.

No. of Threshold (qosIfRedNumThresholdSets)

The values in this entry apply only to queues with the number of thresholds specified by this attribute.

Threshold (qosIfRedThresholdSet)

This table field provides the threshold set to which the lower and upper values apply. It must be in the range of 1 through qosIfRedNumThresholdSets. There must be exactly one PRI for each value in this range.

Lower Threshold (qosIfRedThresholdSetLower)

This table field provides the threshold value below which no packets are dropped.

Upper Threshold (qosIfRedThresholdSetUpper)

This table field provides the threshold value above which no packets are dropped.