# SSL Blade Configuration: Modify VLANs

The Modify SSL BLade dialog box allows you to modify a selected secure socket layer (SSL) VLAN.

## Procedure

1. Right-click the SSL blade, then select SSL Blade Configuration. The SSL Configuration dialog box appears.

2. Select a row, then click Modify.

The following information appears:

SSL VLAN

VLAN ID

IP Address

Subnet Mask

Gateway

Is Admin VLAN?

Static Route

Route IP Address

Route Subnet Mask

Route Gateway

### VLAN ID

Number assigned to a particular VLAN.

### IP Address

IP address of the interface, in A.B.C.D format.

### Subnet Mask

IP mask address associated with a particular VLAN.

### Gateway

IP gateway for the traffic in a particular VLAN.

### Is Admin VLAN?

When true, the VLAN is an admin VLAN.

### Route IP Address

IP Address of the server that is one or more layer 3 hops away from the secure sockets layer (SSL) services module.

### Route Subnet Mask

Subnet Mask of the server that is one or more layer 3 hops away from the secure sockets layer (SSL) services module.

### Route Gateway

Gateway for server that is one or more layer 3 hops away from the secure sockets layer (SSL) Services Module.