# EOU Configurations

## Navigation

Port > Configure > PAE > EOU Configurations

The following information appears:

> Admin Status (cnnEouIfAdminStatus)

> Validation (cnnEouIfValidateAction)

> Fail Policy (cnnEouIfAaaFailPolicy)

### Admin Status (cnnEouIfAdminStatus)

Current administrative status of this interface.

There are three possible values:

> auto: Posture validation via EOU is enabled on this interface if an endpoint device is found.

> disabled: Posture validation via EOU is disabled.

> bypass: The host connected to this interface bypasses posture validation and directly downloads the host network access policy from authentication, authorization, and accounting (AAA) server.

### Validation (cnnEouIfValidateAction)

EOU validation setting configured for the endpoint devices associated with this interface.

Note: This object always returns the value none when read.

There are four possible values:

> none(1): No operation is performed.

> initialize(2): Manually initiates reauthentication of all associated endpoint devices.

> revalidate(3): Revalidates the EOU posture credentials of all associated endpoint devices.

> noRevalidate(4): Disables the revalidation of all associated endpoint devices.

### Fail Policy (cnnEouIfAaaFailPolicy)

The name of the policy template to be applied when cnnEouHostResultState is set to aaaFail. The specified policy name must exist in cpgPolicyTable if it is not an empty string.