# Mobile Network Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Mobile Network Configs from the Category list.

The following information appears:

> Mobile Network Interfaces Index (cmiMrMobNetIfIndex)

> Inet Address (cmiMrMobNetAddr)

> Prefix Length Associated (cmiMrMobNetPfxLen)

> Mobile Network Address Type (cmiMrMobNetAddrType)

> Create/Delete Row (cmiMrMobNetStatus)

> Tunnel Interfaces Index (cmiMrHaTunnelIfIndex)

### Mobile Network Interfaces Index (cmiMrMobNetIfIndex)

The ifIndex value from the Interfaces table of MIB II for the interface on the mobile router connected to the mobile network.

### Inet Address (cmiMrMobNetAddr)

The IP address of the mobile network.

### Prefix Length Associated (cmiMrMobNetPfxLen)

The prefix length associated with the mobile network IP address.

### Mobile Network Address Type (cmiMrMobNetAddrType)

The type of IP address stored in cmiMrMobNetAddr.

### Create/Delete Row (cmiMrMobNetStatus)

The row status for the mobile network entry.

### Tunnel Interfaces Index (cmiMrHaTunnelIfIndex)

The ifIndex value from Interfaces table of MIB II for the tunnel interface (to HA) of the mobile router.