# GGSN GTP Path Table

Use this dialog to view the path details of GGSN with SGSN or charging gateway.

## Procedure

In the Chassis view, right-click the device and select Configure from the popup menu.

The following information appears:

> Address Type (cGtpPathAddressType)

> Address (cGtpPathAddress)

> Port (cGtpPathPort)

> GTP Version (cGtpPathVersion)

### Address Type (cGtpPathAddressType)

Type of Internet address by which cGtpPathAddress is reachable.

### Address (cGtpPathAddress)

An address that uniquely identifies a remote node to which this path is established.

### Port (cGtpPathPort)

Port on the remote node. The value zero is invalid.

### GTP Version (cGtpPathVersion)

GTP version of the path identified by cGtpPathEntry.

Values are:

- version0 represents GTP version 0

- version1 represents GTP version 1.