# GGSN - SGSN Throughput Statistics

## Procedure

1. Right-click the device and then select Monitor.

2. Select GGSN - SGSN Statistics from the Category list.

3. Select a row and click on Monitor.

The following information appears:

> Data Last Collected (cGgsnSgsnThruPutLastCollected)

> Upstream Packets Sent (cGgsnSgsnUpStreamPktCnt)

> Upstream Bytes Sent (cGgsnSgsnUpStreamByteCnt)

> Downstream Packets Sent (cGgsnSgsnDownStreamPktCnt)

> Downstream Bytes Sent (cGgsnSgsnDownStreamByteCnt)

### Data Last Collected (cGgsnSgsnThruPutLastCollected)

This object represents the delta value between the time when this data is collected and the time it is retrieved.

### Upstream Packets Sent (cGgsnSgsnUpStreamPktCnt)

This object represents the total number of upstream packets sent on this SGSN data path. Data flow from MS to PDN is considered to be upstream traffic.

### Upstream Bytes Sent (cGgsnSgsnUpStreamByteCnt)

This object represents the total number of upstream bytes sent on this SGSN data path. Data flow from MS to PDN is considered to be upstream traffic.

### Downstream Packets Sent (cGgsnSgsnDownStreamPktCnt)

This object represents the total number of downstream packets sent on this SGSN data path. Data flow from PDN to MS is considered to be downstream traffic.

### Downstream Bytes Sent (cGgsnSgsnDownStreamByteCnt)

This object represents the total number of downstream bytes sent on this SGSN data path. Data flow from PDN to MS is considered to be downstream traffic.