# RP Update Statistics

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based RP update statistics.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

4. With an entry selected in the PCFs & Service Options table, click RP Update Statistics.

The following information is displayed:

> Updates Transmitted (cCdmaPcfSoRpUpdTxdReqs)

> Updates Accepted (cCdmaPcfSoRpUpdAcptdReqs)

> Updates Denied (cCdmaPcfSoRpUpdDeniedReqs)

> Updates Not Acknowledged (cCdmaPcfSoRpUpdNotAckedReqs)

> Initial Updates (cCdmaPcfSoRpUpdInitTxdReqs)

> Retransmitted Updates (cCdmaPcfSoRpUpdReTxdReqs)

### Updates Transmitted (cCdmaPcfSoRpUpdTxdReqs)

Number of A11 registration update requests transmitted since system startup.

### Updates Accepted (cCdmaPcfSoRpUpdAcptdReqs)

Number of A11 registration update requests received with the Status field set to zero since system startup.

### Updates Denied (cCdmaPcfSoRpUpdDeniedReqs)

Number of A11 registration update requests received with the Status field set to a non-zero value since system startup.

### Updates Not Acknowledged (cCdmaPcfSoRpUpdNotAckedReqs)

Number of A11 registration update requests sent when no corresponding acknowledgements were received since system startup.

### Initial Updates (cCdmaPcfSoRpUpdInitTxdReqs)

Number of initial A11 registration update requests, excluding retransmitted updates, since system startup.

### Retransmitted Updates (cCdmaPcfSoRpUpdReTxdReqs)

Number of retransmitted A11 registration update requests since system startup.