# CDMA PDSN PPP Miscellaneous Stats Contd

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Statistics button.

4. Select category CDMA PDSN PPP Miscellaneous Stats Contd.

5. Select a row and click on Monitor.

The following information appears:

> Compression Negotiation Failure (cCdmaPppCompressNegoFailures)

> LCP Echo Requests Transmitted (cCdmaPppTransmittedEchoReqs)

> LCP Echo Requests Retransmitted (cCdmaPppRetransmittedEchoReqs)

> LCP Echo Reply Received (cCdmaPppReceivedEchoReplies)

> LCP Echo Requests Timed Out (cCdmaPppEchoRequestTimeouts)

> Unidentified Protocol Packets Discarded (cCdmaPppUnknownProtocolPktDiscards)

> Bad Length Packets Discarded (cCdmaPppBadLengthPktDiscards)

### Compression Negotiation Failure (cCdmaPppCompressNegoFailures)

Total number of PPP negotiations that failed due to compression negotiation failure since the system was last restarted.

### LCP Echo Requests Transmitted (cCdmaPppTransmittedEchoReqs)

Total number of LCP Echo requests transmitted since the system was last restarted.

### LCP Echo Requests ReTransmitted (cCdmaPppRetransmittedEchoReqs)

Total number of LCP Echo requests retransmitted since the system was last restarted.

### LCP Echo Reply Received (cCdmaPppReceivedEchoReplies)

Total number of LCP Echo reply received since the system was last restarted.

### LCP Echo Requests Timed Out (cCdmaPppEchoRequestTimeouts)

Total number of LCP Echo requests timed out since the system was last restarted.

### Unidentified Protocol Packets Discarded (cCdmaPppUnknownProtocolPktDiscards)

Total number of packets discarded at PPP stack due to protocol value can not be identified, since the system was last restarted.

### Bad Length Packets Discarded (cCdmaPppBadLengthPktDiscards)

Total number of PPP packets discarded stack due to bad length since the system was last restarted.