# GGSN GTP Director Status

From this dialog box, you can view the current status of the GGSN GTP director.

Note: This dialog is available only if cGtpGSNService is set to gtpdirector.

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Statistics.

4. Select GGSN GTP Director Status from the Category drop-down box.

The following information is displayed:

> Pending create PDP requests (cgdPendingPdps)

> Unique create PDP requests forwarded (cgdCreatePdpRequestFwded)

> Total create PDP requests forwarded (cgdTotalCreatePdpRequestFwded)

> Create PDP requests rejected (cgdCreateRequestRejected)

> Unsupported signaling messages (cgdTotalUnsupportedMessages)

> Total PDP requests dropped (cgdPdpRequestDropped)

### Pending create PDP requests (cgdPendingPdps)

Number of create PDP requests whose connection retry timer has not expired.

### Unique create PDP requests forwarded (cgdCreatePdpRequestFwded)

Number of unique create PDP requests forwarded by the GDM to GGSN. This does not include retransmissions.

### Total create PDP requests forwarded (cgdTotalCreatePdpRequestFwded)

Number of create PDP requests forwarded by the GDM to GGSN. This includes retransmissions.

### Create PDP requests rejected (cgdCreateRequestRejected)

Number of create PDP requests rejected by GGSN.

### Unsupported signaling messages (cgdTotalUnsupportedMessages)

GDM does not support any signalling message other than create PDP request. If the GDM receives any unsupported signalling message, it will not be forwarded to GGSN and will be dropped. cgdTotalUnsupportedMessages gives the total number of unsupported signalling messages received by the GDM.

### Total PDP requests dropped (cgdPdpRequestDropped)

Number of PDP requests dropped by the GDM due to routing failures, which occur if the GTP is unable to pass the packet to IP.