# CDMA PDSN Registration Update Additional Statistics

This dialog box is applicable to Member and Peer to Peer clusters. From here, you can view valid and accepted registration updates.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Registration Update Additional Statistics.

The following data is displayed:

> Registration Update Acks Received (cCdmaRpUpdReceivedAcks)

> Registration Update Acks Discarded (cCdmaRpUpdDiscardedAcks)

> Registration Update Reqs - Lifetime Expiry (cCdmaRpUpdRpLifeExpReqs)

> Registration Update Reqs - PPP Termination (cCdmaRpUpdPPPtermReqs)

> Registration Update Reqs – Other Reason (cCdmaRpUpdOtherReasonReqs)

### Registration Update Acks Received (cCdmaRpUpdReceivedAcks)

Number of A-11 registration acknowledgements received since system startup.

### Registration Update Acks Discarded (cCdmaRpUpdDiscardedAcks)

Number of A-11 registration acknowledgements discarded since system startup.

### Registration Update Reqs - Lifetime Expiry (cCdmaRpUpdRpLifeExpReqs)

Number of initial A-11 registration updates since system startup due to a RP lifetime expiration.

Note: This count does not include any retransmissions.

### Registration Update Reqs - PPP Termination (cCdmaRpUpdPPPtermReqs)

Number of initial A-11 registration updates sent as a result of a PPP termination since system startup.

Note: This count does not include any retransmissions.

The code field in the registration reply message is set to non-zero.

### Registration Update Reqs – Other Reason (cCdmaRpUpdOtherReasonReqs)

Number of initial A-11 registration updates sent due to reasons other than a RP lifetime expiry or PPP termination since system startup.

Note: This count does not include any retransmissions.