# GGSN - SGSN Statistics

## Procedure

1. Right-click the device and then select Monitor.

2. Select GGSN - SGSN Statistics from the Category drop-down box.

The following information appears:

> Remote Address (cGtpPathAddress)

> Remote Port (cGtpPathPort)

> Collection Interval (cGgsnSgsnThruPutInterval)

### Remote Address (cGtpPathAddress)

An address that uniquely identifies a remote node to which this path is established.

### Remote Port (cGtpPathPort)

This object identifies the port on the remote node. The value of zero is invalid.

### Collection Interval (cGgsnSgsnThruPutInterval)

This object should be one of the values set in the objects cGgsnThruputIntervalOne or cGgsnThruputIntervalTwo except for value '0', which means the throughput collection is disabled.