# RS-232 Port Configuration Information

The RS-232 port configuration dialog box shows the following information for an EIA/TA-232 port:

> Index

> Type

> Input Signals

> Output Signals

> Input Speed

> Output Speed

> Output Flow Control

Index (rs232PortIndex)

Specifies a unique value for each port. If possible, index values should map directly to external connectors.

Type (rs232PortType)

Specifies the hardware type.

Input Signals (rs232PortInSigNumber)

Specifies the number of detectable input signals for the port.

Output Signals (rs232PortOutSigNumber)

Specifies the number of output signals the port can assert.

Input Speed (rs232PortInSpeed)

Specifies the input speed of the port in bits per second.

Output Speed (rs232PortOutSpeed)

Specifies the output speed of the port in bits per second.

Output Flow Control

Specifies the type of flow control the port is using.