# Virtual Client Info

This dialog box provides information about the client IP address, client mask, and the range of IP addresses of the clients.

## Procedure

1. Right-click the device, then select Configure > SLB Statistics.

2. With a server load balancing (SLB) instance selected, click Virtual Servers.

3. With an entry selected, click VirClient.

> Client IPAddress (slbVirtualClientIpAddress)

> Client Mask (slbVirtualClientMask)

> Client Range Exclude (slbVirtualClientExclude)

> Virtual Client Row status (slbVirtualClientRowStatus)

### Client IPAddress (slbVirtualClientIpAddress)

The IP address of the client. It is used with the slbVirtualClientMask to represent subsets of client traffic being handled by the virtual server.

### Client Mask (slbVirtualClientMask)

The general purpose mask of the client. It is used with the slbVirtualClientIpAddress to represent subsets of client traffic being handled by the particular virtual server.

### Client Range Exclude (slbVirtualClientExclude)

The truth value that determines whether client range should be included or excluded on the virtual server.

### Virtual Client Row status (slbVirtualClientRowStatus)

The management station uses row status to create or delete the row entry in slbVirtualClientTable following the RowStatus textual convention.