# CDMA PDSN Registration Accepted Stats

This dialog box is applicable to Controller, Member, and Peer to Peer clusters. From here, you can view registration statistics for valid and accepted requests.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Registration Accepted Stats.

The following data is displayed:

> Registration Request Received (cCdmaRpRegReceivedReqs)

> Registration Request Accepted (cCdmaRpRegAcceptedReqs)

> Registration Request for New Connection Accepted (cCdmaRpInitRegAcceptedReqs)

> Registration Request for Refreshing connection Accepted (cCdmaRpReRegAcceptedReqs)

> Registration Request for Disconnection Accepted (cCdmaRpDeRegAcceptedReqs)

### Registration Request Received (cCdmaRpRegReceivedReqs)

Number of A-11 registration requests received since system startup.

### Registration Request Accepted (cCdmaRpRegAcceptedReqs)

Number of A-11 registration requests accepted since system startup.

The code field in the registration reply is set to zero.

### Registration Request for New Connection Accepted (cCdmaRpInitRegAcceptedReqs)

Number of accepted A-11 registration requests since system startup that are used for establishing new R-P connections. These A-11 registration requests contain the connection setup airlink record.

The code field in the registration reply is set to zero.

### Registration Request for Refreshing connection Accepted (cCdmaRpReRegAcceptedReqs)

Number of accepted A-11 registration requests since system startup that are used for refreshing the established R-P connections.

The code field in the registration reply is set to zero.

### Registration Request for Disconnection Accepted (cCdmaRpDeRegAcceptedReqs)

Number of accepted A-11 registration requests since system startup that are used for deactivating the established R-P connections.

The code field in the registration reply is set to zero.