# RP Update Failures

From this dialog box, you can view Packet Control Function (PCF) and Service Option (SO)-based RP update failures.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN PCF & SO Based Statistics.

4. With an entry selected in the PCFs & Service Options table, click RP Update Statistics.

5. Select RP Update Failures.

The following information is displayed:

> Unknown Failures (cCdmaPcfSoRpUpdReaUnSpecFails)

> Administrative Failures (cCdmaPcfSoRpUpdAdmnFails)

> MN Authentication Failures (cCdmaPcfSoRpUpdMNAuthFails)

> ID Mismatch Failures (cCdmaPcfSoRpUpdIdMismatFails)

> Bad Request Failures (cCdmaPcfSoRpUpdBadReqFails)

### Unknown Failures (cCdmaPcfSoRpUpdReaUnSpecFails)

Number of registration updates that failed for an unspecified reason since system startup.

### Administrative Failures (cCdmaPcfSoRpUpdAdmnFails)

Number of registration updates that failed due to administrative prohibition since system startup.

### MN Authentication Failures (cCdmaPcfSoRpUpdMNAuthFails)

Number of registration updates that failed due to a Mobile Node (MN) authentication failure since system startup.

### ID Mismatch Failures (cCdmaPcfSoRpUpdIdMismatFails)

Number of registration updates that failed due to a registration identity mismatch since system startup.

### Bad Request Failures (cCdmaPcfSoRpUpdBadReqFails)

Number of registration updates that failed due to a poorly formed request since system startup.