PATH=/ciscoview/Routershare/card/car00000.htm TITLE=Port Adapters and Service Adapters TEXT=Port Adapters and Service Adapters Port adapters and service adapters can be installed on a variety of devices. (PA) supports one more network interfaces. (SA) provides such as compression encryption for other cards.
PATH=/ciscoview/Routershare/card/car00001.htm TITLE=Port Adapters (PA) TEXT=Port Adapters (PA) Provide individual LAN and WAN interface ports on a 7200 or on a VIP card. Each port adapter has Enabled LEDs, You may have connectors) upgrade more recent release. software IOS specification. CiscoView unknown unsupported by your current Available are: PA-ATM-CES PA-A1-OC3SM (1single-mode port) PA-A1-OC3MM (1multi-mode (45 PA-A34T1IMA PA-A3-4E1XIMA ports) PA-ATMDX-DS3 PA-ATMDX-E3 PA-ATMDX-SML-OC3 single-mode, long-reach PA-ATMDX-SMI-OC3 intermediate-reach PA-ATMDX-MM-OC3 (8-port PA-A3-OC12MM (Multi Mode) PA-A3-OC12SMI (Single Intermediate Reach) (BRI) PA-4B-U PA-8B-S/T Channel) ECPA (ESCON channel) PCPA (Parallel Channelized T1/E1, T2/E2, T3/E3 PA-2CE1/PRI-75 (2.0 (unbalanced) PA-2CE1/PRI-120 PA-2CT1/PRI PA_4CT1_CSU PA_8CT1_CSU PA_8CE1 PA-CT3 interfaces) PA-CE3 PA-MC-T3 PA-MCX-2TE1 MIX-enabled multichannel without CSU/DSU) PA-MC-8TE1+ PRI) PA-8T1 port, configurable (TDM) PA-4T1 Sonet PA-POS-OC3-MM PA-POS-OC3-SM-IR PA-POS-OC3-SM-LR ADM-SRP OC-12/STM-4 Long Ethernet PA-4E1G PA-8E PA-12E/2FE (Dual-wide switching) PA-5E-FL pa-2fe-tx(573) over (fiber), Fast PA-FE-FX MII PA-FE-TX (RJ-45) PA-2FE-TX (full-duplex duplex) PA-2FE-FX FDDI) PA-F-SM (single-mode PA-F-MM (multi-mode) PA-F/FD-SM PA-F/FD-MM PA-100VG Token Ring PA-MC-STM-1SMI STM-1) (HSSI) PA-H PA-2H Inter-Switch Link (ISL) PA-2FEISL-FX Network PA-2FEISL-TX Serial lines) line) PA-2JT2 (HSD 6.312Mbps, PA-1T3 PA-2T3+ PA-T3+ PA-1E3 PA-2E3 PA-4R-FDX PA-4R-DTR Voice Card PA-VXC-2TE1+ PA-VXB-2TE1+ PA-VXA-1TE1-30+ High-Capacity Enhanced Digital channels) PA-VXA-1TE1-24+ providing 155.52Mbps using connector. dual-wide performed routers, fourth (1.54 Mbps) that can both unstructured (n Nx64 kbps) CES, compliant Forum standards, either OC-3 (155 (SM) standards-based interface. single-wide, 1-port (long reach). (intermediate basic incorporates ports, supporting interfaces. The module represents Termination (NT1). provides 16-Kbit/sec 56 Kbit/sec. Status indicated channels. Green Active Black AnyLan otherwise state Adapter. which connections IBM-compatible mainframes. It supports cabling architecture. This technology. parallel (also called bus tag). 2-port (balanced) PA-4CT1-CSU 4-port integrated PA-8CT1-CSU DSX1 like protection. user options configuring T1, fractional ISDN support. 128 usable lines. CSU. PA-8CE1 single-side capability. channelize non-framed supported. inteface Three used external configured timeslots, will test future multi-channel single-width via BNC connectors. group). presented system individually. 8PRI single-port OC3c/STM1 Packet (POS) transceiver 400 Kilometers. range) double-wide twelve 10BT two10/100BT front panel. Layer local destination MAC address hardware. IEEE (802.12 operates 100Mbps data rate, (UTP) cable. defined environment 802.3) (802.5). high-speed ports. inter-virtual (VLAN) bridging routing carry traffic uplink. unshield twisted-pair copper Connects such V.35, telephone Postal Telegraph (PTT) networks, synchronous specified G.703/G.704. point-to-point 7xxx series. from leased-line services. unframed access, 2.048Mbps speeds 75-ohm 120-ohm 15-pin D-shell (DB-15) receptacles 1,984 kbps. terminal equipment (DTE G.703a. Through these 7500. communicate MHz Speed 6.3) ITU Recommendation second-generation versatile processors (VIP2), integrating unit (DSU) functionality into router. improved Processor 802.5r dedicated (DTR) stations concentrator half-duplex operation. (TE) D-channel multi-access. X.21, RS-232 eight If running versions earlier than 11.1(9)CA 11.2(6)P cards shown PA-8T-V35. With later, displays PA-8T-X21 PA-8T-232 correctly. five must exactly operation, falls back RJ-45, whose line. following protocols: EIA/TIA-232 EIA/TIA-449 requires MAU AUI 10BaseT token-ring DB-9 networks. PA-A3-4T1IMA inverse multiplexing (ATM Deluxe) Multimode VIP4 (NPE-300) platforms. AAL5 convergence layer, classes shared runs concatenated complete bandwidth portion it. fiber, WDM wavelength ADM tributary. physical compatible. Hence, dedicates modes same consists counter rotating optic rings. sends direction( down stream its corresponding control information opposite 7000 TDM. 7500/7200 allows become hub. Extended DSP memory. connectivity SDH MIB Enumeration pa-mc-stm1-smi(817) 7200, 7100 contains being ethernet. highly solution division multiplexer processing IP, Frame Relay
PATH=/ciscoview/Routershare/card/car00048.htm TITLE=Fast Ethernet Connectors TEXT=Fast Ethernet Connectors Each FE port adapter has two 100BaseT connectors: A Media Independent Interface (MII) Either can RJ-45 twisted pair (on PA-FE-TX) SC fiberconnector PA-FE-FX) The interfaces FEIP are mounted adapters that attachto motherboard. Only one used operations interface. status of isindicated with LEDs attached Category UTP for 100BaseTX; MIIconnector connected through user-provided transceivers otherphysical layers. Both full-duplex and half-duplex supported.
PATH=/ciscoview/Routershare/card/car00049.htm TITLE=Fast Ethernet LEDs TEXT=Fast Ethernet LEDs In addition to the Enabled LED, a fast Ethernet port adapter has two other LEDs, an MII command either RJ-45 fiber LED. Of these two, one that CiscoView lit, interface indicates which connector configured active port. Note: If FE card, shutdown downloaded (in state), physical does another change reflect status until been used state. When means Is powered full-duplex correctly connected. backplane valid version microcode successfully recognized by (bus for BRI Ports PA-4B-U PA-8B-S/T each channels. (Green) Black Any PHY FDDI station. shuts fails, automatically wraps signal so complete transmission around ring. direction. There are B. both green, then part only wrapped (with LED) down. black, PA-4R-DTR four additional Meaning INS inserted into token 4/16 Mbps operating Megabits second. CPA-LEDs ECPA, PCPA, Present presence path type. this ESCON Channel Adapter. Parallel tag). Loaded daughterboard executing. Light seen synchronization established. (ECPA) Operational out sensed. (PCPA). Online least channel. PCA will response device address.
PATH=/ciscoview/Routershare/card/car00056.htm TITLE=High Speed Serial Interface (HSSI) TEXT=High Speed Serial Interface (HSSI) Provides one or two HSSI ports (up to 52 Mbps). Each port allows you choosefrom range softwareconfiguration. connectivity options, including ATM, SMDS, Frame Relay, orprivate lines. these can be configured speeds DS3(45 Mbps) E3 (34 Mbps). different network connections required only cable is for port.
PATH=/ciscoview/Routershare/card/car00062.htm TITLE=Service Adapters (SA) TEXT=Service Adapters (SA) Provide specialized network services on a 7200 or on a VIP or VIP2 card, as follows: CSA (Compression Adapter) (ESA) (Encryption SA-ISA (Integrated Port (VAM) (VPN) Acceleration Module) (CSA) Provides decompression Standard (in hardware) information multiple applications. concurrently. Can interface with routers. that only supports software compression. addition Predictor), algorithms used (Stac Novell Magnalink Scalable Algorithm (MSA) IBM Advanced Loss Data (ALDC). CiscoView before monitor: statistics configuration There three LEDs the Adapter: Meaning if Lit (Green) Enabled enabled. Error Not supported. adapter high-performance, hardware-assisted tunneling encryption. remote access site-to-site intranets extranets. both IPSec Point-to-Point Protocol/Microsoft (PPTP/MPPE). SM-ISM Hardware accelerator compression, slot. 40/56-bit 7100. series. May (DES) 30 Mbs 7500 Series Install any PA chassis. one (VIP2-40 later). adjacent also available devices it. You have upgrade more recent release IOS unknown unsupported encryption, key generation, suitable virtual private Triple (3DES) greater than full-duplex DS-3 Online (up 145 Mbps) VPNs such Moreover, 5000 encrypted tunnels mixed environments requirements. integrates RSA (IPPCP) Layer Accelerating processing speeds setup creation time improving overall initialization. And those where bandwidth costly, hardware-based Payload Lempel-Ziv-Stac (LZS) traffic sent pay-per-byte WAN connections. SM-VAM, installs module SA-VAM, Card image installed package. Connection (CCO) http://www.cisco.com about upgrading recognizes but does yet support. your
PATH=/ciscoview/Routershare/card/car00065.htm TITLE=Versatile Interface Processor (VIP) TEXT=Versatile Interface Processor (VIP) The VIP card (VIP, VIP-2, or VIP-2-50) uses a single motherboard with one networks replaceable supports adapters. (PA) quality-of-service (SA) card. Any combinations of cards significantly Label installed first-generation following: Ethernet (10BaseT), Fast (100BaseTX), Serial, Random Token Ring ports: PAs VIP4 Distributed fourth high-performance, 7500 series routers. based 250MHz R7000 MIPS microprecessor system controller ASIC. primary features are: RM7000 CPU. Support legacy Non-distributed versions. Large memory configuration. (VIP6-80) Cisco Services Accelerator provides 40 percent improvement over more than VIP2-50 when (QoS) enabled. interface. such, ideal enterprise provider customers who require high-speed interfaces. applications. that highest-speed OC-12 OC-3 ATM channelized STM-1 combined Layer 3-7 these Performance enhanced certain Examples some include Committed Access Rate (dCAR) Weighted Fair Queuing (dWFQ) Early Detection (dWRED) Traffic Shaping (dTS) Network-Based Application Recognition (dNBAR) Multiprotocol Switching (MPLS) Virtual Private Networking (VPN) +
PATH=/ciscoview/Routershare/card/car00070.htm TITLE=Add in next release TEXT=Add in next release Add the following links to topic #2 under Channelized T1/E1, T2/E2, T3/E3. The popup topics which they are already present, but inaccessible card.hlp. PA-8CT1-CSU (8 ports) PA-8CE1 channelized, BRI, non-framed) PA-4CT1-CSU (4 fractional, BRI)
PATH=/ciscoview/Routershare/card/car00074.htm TITLE=FDDI Interface TEXT=FDDI Interface A 100Mbps FDDI LAN network interface using fiber optic cable. There are three LEDs on each card, labeled PHY B standby Enabled If the router administrative running IOS version 10.2 earlier, status color based port&#146;s (ifAdminStatus) operational (ifOperStatus) values, same both connectors. 10.3 later Port (fddimibPORTConnectState) State for separately, with following possible values: brown disabled blue connecting green active
