# GGSN PLMN Table

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.

2. Select MWAM module from the Category drop-down box.

3. With a device selected in the MWAM module dialog box, click Configure.

4. Select GGSN PLMN Table from the Category drop-down box.

The following information appears:

> Mobile Country Code (MCC) (cGgsnPlmnMcc)

> Mobile Network Code (MNC) (cGgsnPlmnMnc)

> PLMN Scope (cGgsnPlmnScope)

### Mobile Country Code (MCC) (cGgsnPlmnMcc)

Segment of the Public Land Mobile Network (PLMN) ID that indicates the relevant Mobile Country Code.

### Mobile Network Code (MNC) (cGgsnPlmnMnc)

Segment of the PLMN ID that indicates the relevant Mobile Network Code.

### PLMN Scope (cGgsnPlmnScope)

Indicates the scope of the PLMN. There are two possible values:

> home

> trusted

Note: At any given time, only one PLMN entry can have the value home.