# Receive Side High Priroity Traffic Statistics

Dilog box displays following information:

Unicast High Priority Packets (srpHostIntUcastHighPriPktsIn)

UniCast High Priority Octets (srpHostIntUcastHighPriOctetsIn)

MultiCast High Priority Packets (srpHostIntMcastHighPriPktsIn)

MultiCast High Priority Octets (srpHostIntMcastHighPriOctetsIn)

Unicast High Priority Packets (srpHostIntUcastHighPriPktsIn)

Number of high priority unicast packets received from higher layer during a 15-minute interval during the past 24 hours.

UniCast High Priority Octets (srpHostIntUcastHighPriOctetsIn)

Number of high priority unicast octets received from higher layer during a 15-minute interval during the past 24 hours.

MultiCast High Priority Packets (srpHostIntMcastHighPriPktsIn)

Number of high priority multicast packets received from higher layer during a 15-minute interval in the past 24 hours.

MultiCast High Priority Octets (srpHostIntMcastHighPriOctetsIn)

Number of high priority multicast octets received from higher layer during a 15-minute interval during the past 24 hours.