# Displaying IP Configuration for a CIP Port

To display the IP configuration of a CIP port from the CiscoView Configure Port window, select IP Config from the CATEGORY popup menu. The following information is displayed:

IP Address (sysIpAddr)

Subnet Mask (sysNetMask)

Broadcast Address (sysBroadcast)

# IP Address (sysIpAddr)

Specifies the IP address of the displayed device.

# Subnet Mask (sysNetMask)

Specifies the network mask for the displayed device.

# Broadcast Address (sysBroadcast)

Specifies the broadcast address for the displayed device.