# RP Registration Request Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select CDMA PDSN PCF & SO Based Statistics from the Category list.
3. Select a row and click the RP Registration Statistics button.
4. Select RP Registration Request Statistics from the Category list.

The following information appears:

> Initial A11 Registration Requests (cCdmaPcfSoRpInitRegRcvdReqs)

> A11 Re-registration Request (cCdmaPcfSoRpReRegRcvdReqs)

> A11 De-registration Request (cCdmaPcfSoRpDeRegRcvdReqs)

> Handoff Registration Request (cCdmaPcfSoRpHandoffRegRcvdReqs)

> Airlink Start Re-registration Request (cCdmaPcfSoRpReRegAirlinkStarts)

> Airlink Stop Re-registration Request (cCdmaPcfSoRpReRegAirlinkStops)

> Airlink Stop De-registration Request (cCdmaPcfSoRpDeRegAirlinkStops)

### Initial A11 Registration Requests (cCdmaPcfSoRpInitRegRcvdReqs)

The number of initial A11 registration requests received since the system was last restarted.

### A11 Re-registration Request (cCdmaPcfSoRpReRegRcvdReqs)

The number of A11 re-registration requests received since the system was last restarted.

### A11 De-registration Request (cCdmaPcfSoRpDeRegRcvdReqs)

The number of A11 de-registration requests received since the system was last restarted.

### Handoff Registration Request (cCdmaPcfSoRpHandoffRegRcvdReqs)

The number of A11 handoff registration requests received since the system was last restarted.

### Airlink Start Re-registration Request (cCdmaPcfSoRpReRegAirlinkStarts)

The number of A11 re-registration requests containing Airlink Start since the system was last restarted.

### Airlink Stop Re-registration Request (cCdmaPcfSoRpReRegAirlinkStops)

The number of A11 re-registration requests containing Airlink Stop since the system was last restarted.

### Airlink Stop De-registration Request (cCdmaPcfSoRpDeRegAirlinkStops)

The number of A11 de-registration requests containing Airlink Stop since the system was last restarted.