# BGP Policy Accounting Traffic

The BGP Policy Accounting Traffic Monitor dialog box monitors a particular type of traffic on a particular interface.

## Procedure

For CiscoView versions earlier than 5.2:

1. Right-click the device. Then select Configure, or double-click the device. The Device Configuration dialog box appears.

2. Select Protocols from the Category list.

3. Select BGP4 in from the SelectProtocol list. Then click the Details button. The BGP4 Configuration dialog box appears.

4. Select BGP4 Peer Information from the Category list.

5. Select a row from the table and click the Monitor button. The Monitor BGP4 Traffic dialog box appears.

6. Select BGP4 Policy Accounting Traffic from the Category list.

For CiscoView version 5.2 and later:

1. Right-click the device. Then select Configure, or double-click the device. The Device Configuration dialog box appears.

2. Select Protocols from the Category list.

3. Select BGP4 in the Selectprotocol list, then click the Details button. The BGP4 Configuration dialog box appears.

> > Note: The left frame in the dialog box displays the categories and the right frame displays the category details or a table. If a table is displayed, the variable on which the table is indexed and the key values of the index are listed below the category. Double-click the category to view the table and double-click a key value to view details of a particular row in the table.

> > Multiple indexes for a table, if any, are listed below the category in a nested manner. Select a key value to view the rows of the table about that value. Select a key value of the lowest indexing variable to view the details of that particular row.

4. Select BGP4 Peer Information from the left pane of the BGP4 Configuration dialog box. A table appears on the right pane of the dialog box.

5. Select a row in the table and click the Monitor button. The Monitor BGP4 Traffic dialog box appears.

6. Select BGP4 Policy Accounting Traffic from the Category list.

The following information appears:

Received Packets (cbpAcctInPacketCount)

Received Octets (cbpAcctInOctetCount)

## Related Topics

BGP4 Messages

BGP4 FSM Transitions

### Received Packets (cbpAcctInPacketCount)

Total number of packets of a particular traffic type received on an interface.

### Received Octets (cbpAcctInOctetCount)

Total number of octets of a particular traffic type received on an interface.