# RSVP Neighbor Table

The table displays the following details:

Neighbor Address (rsvpNbrAddress)

Neighbor Protocol (rsvpNbrProtocol)

Neighbor Status (rsvpNbrStatus)

### Neighbor Address (rsvpNbrAddress)

The IP4 or IP6 address used by a neighbor. This object may not be changed when the RowStatus is active.

### Neighbor Protocol (rsvpNbrProtocol)

The encapsulation used by the neigbor.

### Neighbor Status (rsvpNbrStatus)

The status of neighbors. Active for all neighbors.

Neighbor Status is used for configuring neighbors. In the presence of configured neighbors, the implementation might limit the set of valid neighbors to those already configured.