# SSL Blade Configuration: Configure VLANs

The SSL Blade Configuration dialog box displays the VLANs configured on the secure sockets layer (SSL) blade.

## Procedure

1. Right-click the SSL blade, then select SSL Blade Configuration.

The following information appears:

VLAN ID

IP Address

Subnet Mask

Gateway

Route IP Address

Route Subnet Mask

Route Gateway

Is Admin VLAN?

From the SSL Configuration dialog box:

To create a new server load balancing VLAN, click Create.

To delete a VLAN, select a row, then click Delete.

To modify a VLAN, select a row, then click Modify.

### VLAN ID

Number assigned to a particular VLAN.

### IP Address

IP address of the interface, in A.B.C.D format.

### Subnet Mask

IP mask address associated with a particular VLAN.

### Gateway

IP gateway for the traffic in a particular VLAN.

### Route IP Address

IP Address of the server that is one or more layer 3 hops away from the secure sockets layer (SSL) services module.

### Route Subnet Mask

Subnet Mask of the server that is one or more layer 3 hops away from the secure sockets layer (SSL) services module.

### Route Gateway

Gateway for server that is one or more layer 3 hops away from the secure sockets layer (SSL) Services Module.

### Is Admin VLAN?

When true, the VLAN is an admin VLAN.