# Configuration Status

The values of Configuration Status objects reflect the status of configuration database.

To access the dialog box:

> 1. Right-click on the device and select configure from the popup menu. The device configuration information appears.

> 2. Select Configuration Status from the category drop-down list box.

The following information appears:

> Running Last Changed (ccmHistoryRunningLastChanged)

> Running Last Saved (ccmHistoryRunningLastSaved)

> Startup Last Changed (ccmHistoryStartupLastChanged)

> Maximum Event Entries (ccmHistoryMaxEventEntries)

> Entries Bumped (ccmHistoryEventEntriesBumped)

This category is available only on devices that support Cisco IOS Release 11.1 or later.

Running Last Changed (ccmHistoryRunningLastChanged)

The value of sysUpTime when the running configuration was last changed.

If the value of ccmHistoryRunningLastChanged is greater than ccmHistoryRunningLastSaved, the configuration has been changed but not saved.

Startup Last Changed (ccmHistoryStartupLastChanged)

The value of sysUpTime when the startup configuration was last written to. In general, this value is the default configuration that you use when cold starting the system. It could have been changed by a save of the running configuration or by a copy from elsewhere.

Running Last Saved (ccmHistoryRunningLastSaved)

The value of sysUpTime when the running configuration was last saved (written).

If the value of ccmHistoryRunningLastChanged is greater than that for ccmHistoryRunningLastSaved, the configuration has been changed but not saved.

Maximum Event Entries (ccmHistoryMaxEventEntries)

The maximum number of entries that can be held in ccmHistoryEventTable. The recommended value is 10.

Entries Bumped (ccmHistoryEventEntriesBumped)

The number of times the oldest entry in ccmHistoryEventTable was deleted to make room for a new entry.