# CDMA PDSN Fail History Table

Use this option to view CDMA PDSN failure history.

## Procedure

To access CDMA PDSN fail history table information:

Right-click the device and select Configure from the popup menu.

CDMA PDSN Fail History Table dialog box displays:

Index (cCdmaFailSessionIndex)

MS Identifier (cCdmaFailSessionMsid)

MSID Type (cCdmaFailSessionMsidType)

Electronic Station Number (cCdmaFailSessionEsn)

HA IpAddress (cCdmaFailSessionA11HaIp)

FA IpAddress (cCdmaFailSessionA11FaIp)

Connection ID (cCdmaFailSessionConnId)

Session Key (cCdmaFailSessionKey)

Failure Date & Time (cCdmaFailHistFailTime)

Failure Type (cCdmaFailHistFailType)

## Related Topics

CDMA PDSN System Information

CDMA PDSN PCF Table

CDMA PDSN IP Flows Table

CDMA PDSN Session Table

### Index (cCdmaFailSessionIndex)

A unique monotonically incrementing entry identifier. The entry wraps to zero.

### MS Identifier (cCdmaFailSessionMsid)

Mobile station MSID of failed session.

### MSID Type (cCdmaFailSessionMsidType)

Type of MSID of a mobile station that had a failed session.

### Electronic Station Number (cCdmaFailSessionEsn)

Mobile user serial number of failed session.

### HA IpAddress (cCdmaFailSessionA11HaIp)

MoIP home agent address on A11 interface of failed session.

### FA IpAddress (cCdmaFailSessionA11FaIp)

MoIP foreign agent address on A11 interface of failed session.

### Connection ID (cCdmaFailSessionConnId)

Connection ID of failed session.

### Session Key (cCdmaFailSessionKey)

GRE session identification key of failed session.

### Failure Date & Time (cCdmaFailHistFailTime)

Date and time failure occurred.

### Failure Type (cCdmaFailHistFailType)

Failure type of current record.