# RP Update Statistics Contd

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select CDMA PDSN PCF & SO Based Statistics from the Category list.
3. Select a row and click the RP Update Statistics button.
4. Select RP Update Statistics Contd from the Category list.

The following information appears:

> Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdPcfHandoffs)

> Unacknowledged Registration Updates (cCdmaSoRpUpdHandoffNotAckedReqs)

> Acknowledged Registration Updates (cCdmaSoRpUpdHandoffReceivedAcks)

> Accepted Registration Updates (cCdmaSoRpUpdHandoffAcceptedReqs)

> Denied Registration Updates (cCdmaSoRpUpdHandoffDeniedReqs)

> Acknowledgements Discarded (cCdmaSoRpUpdHandoffDiscardedAcks)

> Initial Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdHandoffInitTxdReqs)

> Initial Retransmitted Update Registrations (cCdmaSoRpUpdHandoffReTxdReqs)

### Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdPcfHandoffs)

The number of update registrations sent as a result of inter PCF handoffs since the system was last restarted.

### Unacknowledged Registration Updates (cCdmaSoRpUpdHandoffNotAckedReqs)

The total number of A11 registration updates (sent as a result of inter PCF handoffs) for which no corresponding A11 registration acknowledgements have been received since the system was last restarted.

### Acknowledged Registration Updates (cCdmaSoRpUpdHandoffReceivedAcks)

The total number of A11 registration acknowledgements received for the A11 registration updates that were sent as a result of inter PCF handoffs since the system was last restarted.

### Accepted Registration Updates (cCdmaSoRpUpdHandoffAcceptedReqs)

The total number of A11 registration acknowledgements received with the Status field set to zero, which indicates that the corresponding registration update was accepted, since the system was last restarted.

### Denied Registration Updates (cCdmaSoRpUpdHandoffDeniedReqs)

The total number of A11 registration acknowledgements received with the Status field set to non-zero, which indicates that the corresponding registration update was denied, since the system was last restarted.

### Acknowledgements Discarded (cCdmaSoRpUpdHandoffDiscardedAcks)

The total number of A11 registration acknowledgements discarded since the system was last restarted.

### Initial Inter Pcf Handoff Update Registrations (cCdmaSoRpUpdHandoffInitTxdReqs)

The total number of initial A11 registration updates sent as a result of inter PCF handoffs, excluding the re-transmitted A11 registration updates, since the system was last restarted.

### Initial Retransmitted Update Registrations (cCdmaSoRpUpdHandoffReTxdReqs)

The total number of re-transmitted A11 registration updates sent because the initial registration update (sent as a result of inter PCF handoffs) was not acknowledged or denied since the system was last restarted.