# Power Details

## Navigation

Inline power port > Configure > Inline Power… > Power Details

The following information is displayed:

> Discover Mode (cpeExtPsePortDiscoverMode)

> Powered Device Detected (cpeExtPsePortDeviceDetected)

> IEEE Power Device (cpeExtPsePortIeeePd)

> Default Power Allocated (cpeExtDefaultAllocation)

> Maximum Power (cpeExtPsePortPwrMax)

> Allocated Power (cpeExtPsePortPwrAllocated)

> Available Power (cpeExtPsePortPwrAvailable)

> Actual Power Consumption (cpeExtPsePortPwrConsumption)

### Discover Mode (cpeExtPsePortDiscoverMode)

Discovery mode used by the system to discover the powered device (PD). There are five possible values:

> unknown—the discovery mode on the interface is unknown

> off—indicates that discovery is disabled on the interface

> ieee—the discovery mode on the interface is IEEE-based

> cisco—the discovery mode on the interface is Cisco-based

> ieeeAndCisco—the discovery mode on the interface is both IEEE and Cisco-based

### Powered Device Detected (cpeExtPsePortDeviceDetected)

When the value of this object is true, it indicates that a PD has been detected on the interface.

### IEEE Power Device (cpeExtPsePortIeeePd)

When the value of this object is true, it indicates that the PD attached to the interface is an IEEE-compliant PD.

Note: When the value of this object is false, the value of pethPsePortPowerClassifications (the corresponding object from pethPsePortTable) is irrelevant.

### Default Power Allocated (cpeExtDefaultAllocation)

Indicates the default inline power allocation per port. This is a global configuration parameter that applies to all inline power-capable ports in the system.

Note: The system must consider this object and the per-port configuration object, cpeExtPsePortPwrMax, when determining how much power to allocate to a port. The system will use the lower of the two values.

### Maximum Power (cpeExtPsePortPwrMax)

Maximum amount of power that the power source entity (PSE) will make available to the PD connected to this interface.

### Allocated Power (cpeExtPsePortPwrAllocated)

Amount of power allocated by the PSE to the PD.

### Available Power (cpeExtPsePortPwrAvailable)

Amount of power available for the PD to use. This value may differ from the value of cpeExtPsePortPwrAllocated, depending on how efficiently the PSE delivers power to the PD.

Note: When sufficient power is available to power a PD, the value of this object should be equal to the lesser of the cpeExtDefaultAllocation and cpeExtPsePortPwrMax objects.

### Actual Power Consumption (cpeExtPsePortPwrConsumption)

Actual power consumption of the PD connected to this interface. It may not equal the value of cpeExtPsePortPwrAvailable.