# PSD Server

1. Right click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. elect category PSD Server.

The following information appears:

> Data-Store Name (cPsdClientDSName)

> PSD Server Address Type (cPsdClientDSServerAddressTyp)

> PSD Server Address (cPsdClientDSServerAddress)

> Write/Retrievable Service (cPsdClientDSRetrieveOnly)

> Server Row Status (cPsdClientDSServerRowStatus)

### Data-Store Name (cPsdClientDSName)

Name of the configured data-store.

### PSD Server Address Type (cPsdClientDSServerAddressTyp)

Type of Internet address of the PSD server.

### PSD Server Address (cPsdClientDSServerAddress)

Internet address of the PSD server.

### Write/Retrievable Service (cPsdClientDSRetrieveOnly)

Indicates whether the PSD server can be configured as retrievable only or as write/retrievable . When set to true, the PSD server (the value of the corresponding instance of cPsdClientDSServerAddress) cannot be used for writing Call Detail Records (CDRs). When set to false, the PSD server can be used for writing CDRs as well as retrieving them.

### Server RowStatus (cPsdClientDSServerRowStatus)

Creates a row or deletes an existing row in a table.