# Physical

Device>Configure>Physical

Physical information about the device includes chassis model, power supply, and fan descriptions. This information is often required when troubleshooting.

The CiscoView Physical window displays the following information:

Model (chassisModel)

Manufacturer’s model number for the chassis.

Major Alarm (chassisMajorAlarm)

Whether the chassis major alarm is on or off.

Minor Alarm (chassisMinorAlarm)

Whether the chassis minor alarm is on or off.

Temperature Alarm (chassisTempAlarm)

Whether the chassis temperature alarm is on or off.

Fan Status (chassisFanStatus)

Status of the chassis fan. Possible values are as follows:

Minor fault or the number 3 indicates a minor problem with the power supply.

Major fault or the number 4 indicates a major problem with the power supply.

Other indicates that the status is none of the above.

If the status is not OK, the Fan Errors field gives more information about the power supply failure condition. Possible errors are 12V+ Bad or 12V- Bad.

Fan Diagnostic Errors (chassisFanTestResult)

Test result for the chassis fan. A zero indicates that the supply passed all tests. Bits set in the result indicate error conditions. Possible errors are Temp High, Fan1 Bad, or Fan2 Bad.

Traffic Peak % (sysTrafficPeak)

Highest percentage of traffic relative to a maximum of 100% on the specified device since it was last rebooted.

Traffic Peak Time (sysTrafficPeakTime)

Date and time that the traffic peak occurred.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.