# CDMA PDSN Registration Accepted Statistics

Use this option to view registration statistics of valid and accepted requests.

## Procedure

To access registration statistics information:

1. Right-click the device and select Monitor from the popup menu.

> > Monitor device dialog box appears.

2. Select CDMA PDSN Registration Accepted Stats from the Category menu.

Registration Statistics dialog box displays:

Registration Request Received (cCdmaRpRegReceivedReqs)

Registration Request Accepted (cCdmaRpRegAcceptedReqs)

Registration Request for New Connection Accepted (cCdmaRpInitRegAcceptedReqs)

Registration Request for Refreshing connection Accepted (cCdmaRpReRegAcceptedReqs)

Registration Request for Disconnection Accepted (cCdmaRpDeRegAcceptedReqs)

### Registration Request Received (cCdmaRpRegReceivedReqs)

Number of A-11 registration requests received since system startup.

### Registration Request Accepted (cCdmaRpRegAcceptedReqs)

Number of A-11 registration requests accepted since system startup.

The code field in the registration reply is set to zero.

### Registration Request for New Connection Accepted (cCdmaRpInitRegAcceptedReqs)

Number of accepted A-11 registration requests since system startup that are used for establishing new R-P connections.

These A-11 registration requests contain the connection setup airlink record.

The code field in the registration reply is set to zero.

### Registration Request for Refreshing connection Accepted (cCdmaRpReRegAcceptedReqs)

Number of accepted A-11 registration requests since system startup that are used for refreshing the established R-P connections.

The code field in the registration reply is set to zero.

### Registration Request for Disconnection Accepted (cCdmaRpDeRegAcceptedReqs)

Number of accepted A-11 registration requests since system startup that are used for deactivating the established R-P connections.

The code field in the registration reply is set to zero.