# Interface Address Assignment

## Navigation

To access the Interface Address Assignment dialog box:

1. Right-click the device.

2. Select Configure > Interface Address Table

The following information is displayed:

- Internet address Type (ciiIPAddressType)

- Internet Protocol address (ciiIPAddress)

- Interface Index (ciiIPAddressIfIndex)

- Prefix Length (ciiIPAddressPrefixLength)

- Broadcast Address (ciiIPAddressBroadcast)

- IP Address Category (ciiIPAddressCategory)

### Internet address Type (ciiIPAddressType)

Indicates the Internet address type for this entry's InetAddress and InetAddressPrefixLength objects.

### Internet Protocol address (ciiIPAddress)

IP address to which this entry's addressing information pertains.

### Interface Index (ciiIPAddressIfIndex)

Index value which uniquely identifies the interface to which this entry is applicable. The value of this object is the same as the ifIndex value for the interface associated with this entry.

### Prefix Length (ciiIPAddressPrefixLength)

Length of the prefix associated with this entry's IP address.

- When this object is set to zero, all addresses match.

- The address type is specified by the value of ciiIPAddressType for this entry.

### Broadcast Address (ciiIPAddressBroadcast)

Broadcast address associated with this entry's IP address. The address type is specified by the value of ciiIPAddressType for this entry.

### IP Address Category (ciiIPAddressCategory)

Indicates this entry's IP address category. When setting this object, it must comply with the value of ciiIPAddressCategoryCap.