# Access Port CLI Summary

The CLI Summary option of the VPN Service Blade Access Port Mode Setup Wizard dialog box enables you to view the CLI commands used to configure the VLAN configuration port in the access mode.

## Procedure

1. Right-click on the IPSec VPN Service Blade, then select VPN Service Blade Setup Wizard.

2. Click Create. The IPSec VLAN Configuration dialog box appears.

3. Select the radio button Access Port Mode, then click Configure.... The VPN Service Blade Access Port Mode Setup Wizard dialog box appears.

4. Select a VLAN from the table or create a new VLAN.

5. Click Next. The Outside Access Port option appears.

6. Click Next. A summary of the CLI commands used is displayed.

7. Click Finish to configure the port.