# Voltage Status

The Voltage Status dialog monitors the voltage levels on Network Processing Engine (NPE-G100) or on Network Services Engine (NSE-100) on a CISCO 7304 device.

## Procedure

1. Right-click the chassis, then select Monitor.

2. Select Voltage Status from the drop-down list.

The voltage levels are measured at various test points.

The test points on NSE are:

- NSE outlet 1.8 V (NSE outlet 1.8V)

- NSE outlet 2.5 V (NSE outlet 2.5V)

- NSE outlet 3.3 V (NSE outlet 3.3V)

- NSE outlet 5 V (NSE outlet 5V)

- NSE outlet 12 V (NSE outlet 12V)

- NSE inlet 1.8 V (NSE inlet 1.8V)

- NSE inlet 3.3 V (NSE inlet 3.3V)

- NSE hotspot 1.8 V (NSE hotspot 1.8V)

- NSE db 1.65 V (NSE db 1.65V)

- NSE db 1.8 V (NSE db 1.8V)

The test points on NPE-G100 are:

- NPE outlet 2.5 V ( NPE outlet 2.5 V )

- NPE outlet 3.3 V ( NPE outlet 3.3 V )

- NPE outlet 5.0 V ( NPE outlet 5.0 V )

- NPE outlet 12.0 V ( NPE outlet 12.0 V )

- NPE outlet 3.3c V ( NPE outlet 3.3c V )

- NPE inlet 1.5 V ( NPE inlet 1.5 V )

- NPE outlet 1.8 V ( NPE outlet 1.8 V )

- NPE outlet 1.2 V ( NPE outlet 1.2 V )

- NPE outlet 1.2c V ( NPE outlet 1.2c V )